******************************************************************************
                          SCREW CONNECTION WITH NUT
******************************************************************************
 DEFINITION OF CONNECTION

ZAVRTANJSKA VEZA KRUTE SPOJNICE  
******************************************************************************
  DEFINITION OF CONNECTION
==============================================================================
  THREAD

 Basic Diameter of Screw                         d =      14.000         mm
 Pitch of Thread                                 P =       2.000         mm

 Coefficient of Friction in Thread             miG =       0.150         
------------------------------------------------------------------------------
  SCREW       ISO 4014 - M14 x 70

 Length of Screw                                 l =      70.000         mm
 Length of Thread                                b =      34.000         mm
 Height of Head                                  h =       8.800         mm
 Size of Screw-Wrench                           sw =      21.000         mm
 Inner Diameter of Face under Head              da =      14.000         mm
 Outer Diameter of Face under Head              dw =      21.000         mm
 Heigth of Press Face                           hw =       0.600         mm

 Partitions of Screw
 1. Partition
           Length                               ls =      36.000         mm
           Diameter                             ds =      14.000         mm

 Property Class acc.DIN                         10.9       Rolled
 Yield Stress                                 Rp02 =     900             N/mm^2
 Tensile Strength                               Rm =    1000             N/mm^2
 Shear Strength                                 Tb =     620             N/mm^2
 Modulus of Elasticity                           E =  205000             N/mm^2

 Coefficient of Friction under Head            miK =       0.120
 Coefficient of Usage Rp02                      ni =       0.900
------------------------------------------------------------------------------
  WASHERS UNDER HEAD OF SCREW                 Not Defined

------------------------------------------------------------------------------
  COUPLED MATERIALS
 1. Plate
          Material                                                                 
          Thickness                              h =      21.000         mm
          Allowed Surface Pressure              pG =     490             N/mm^2
          Modulus of Elasticity                  E =  210000             N/mm^2
          Tensile Strength                      Rm =     340             N/mm^2
          Shear Strength                        Tb =     200             N/mm^2
 2. Plate
          Material                                                                 
          Thickness                              h =      26.000         mm
          Allowed Surface Pressure              pG =     630             N/mm^2
          Modulus of Elasticity                  E =  205000             N/mm^2
          Tensile Strength                      Rm =     700             N/mm^2
          Shear Strength                        Tb =     460             N/mm^2

 Diameter of Hole for Screw                     dh =      16.000         mm
 Chamfer under Head of Screw                    fs =       0.000         mm
 Chamfer under Nut                              fn =       0.000         mm
 Left Gap                                       gl =       0.000         mm
 Right Gap                                      gr =      29.000         mm
------------------------------------------------------------------------------
 CONTACT AREA                                      Cut-Out of Ring

 Outer Diameter of Ring                         ro =     106.000         mm
 Outer Diameter of Ring                         ri =      59.000         mm
 Pitch Diameter of Screws                       rs =      80.912         mm
 Angle of Cut-Out of Ring                      ang =      60.000         deg

 Max.Diameter for Press                         Dk =      39.907         mm
 Moment of Inertia of Cont. Ar.                IBT =  711164.269         mm^4

 Coefficient of Friction in Cont. Ar.           mt =       0.150
------------------------------------------------------------------------------
 WASHER UNDER NUT                                 

 Inner Diameter                                 da =      13.000         mm
 Outer Diameter                                 dw =      24.000         mm
 Height of Washer                                h =       2.500         mm
 Modulus of Elasticity                           E =  210000             N/mm^2
 Material                                         S235JR
------------------------------------------------------------------------------
  NUT                                              ISO 4032 - M14

 Inner Diameter of Face under Head              da =      14.000         mm
 Outer Diameter of Face under Head              dw =      19.600         mm
 Height of Nut                                   h =      12.800         mm
 Size of Screw-Wrench                           SW =      21.000         mm

 Material of Nut                            The Same Like Screw                
==============================================================================
    DEFORMATION PROPERTIES
==============================================================================
 Elastic Malleability of Screw              DeltaS =       2.450745e-006 mm/N
 Elastic Malleability of Plates             DeltaT =       4.950806e-007 mm/N
 Bending Elastic Malleab. of Screw           BetaS =       2.367185e-007 mm/N

 Roughness                                      Rz>=        6.000        micro m
 Settlement                                    fz  =      28.000         micro m
------------------------------------------------------------------------------
==============================================================================
                                   LOADS
==============================================================================
 Axial Force                         static     FB =       0.000         kN
 Permanent Additional Force                    FAz =       0.000         kN
 Shear Force                                    FQ =       0.000         kN
 Torsion Moment                                  T =     200.000         Nm
 Inner Press of Connection                      pi =       0.000         N/mm^2

 Position of Axial Force
   -Horizontal Dimension                        as =      22.000         mm
   -Vertical Dimension              Up         hk1 =      15.000         mm
   -                                Down       hk2 =      20.000         mm
 Vertical Position of Axial Force                n =       0.500
 Radius of Torsion Moment                        R =      70.000         mm
 Force Ratio                                    fi =       0.119
==============================================================================
                          TIGHTEN
==============================================================================
 Tightening Moment                              MA =     124.646         Nm
 Mounting Preload                              FVM =      51.395         kN
 Allowed Mounting Force                      FVMal =      72.637         kN
 Necessary Mounting Preload                 FVMmax =      51.395         kN
 Coefficient of Tightening                      kA =       1.800
 What Tighten                                      Nut                 
 How Tighten                                       Elastic             
==============================================================================
                    FORCES, TENSIONS AND STRESSES
==============================================================================
 Screw

 Dynamic Stress                             Sigmaa =         -
 Allowed Dynamic Stress                     SigmaA =      78             N/mm^2
 Equivalent Stress                            Sred =     538             N/mm^2
 Shear Stress                                  Tau =      25             N/mm^2
 Force that the Screw Carries                  FBS =       0.000         kN
 Total Force in Screw                           FS =      51.395         kN
 Settlement                                     FZ =       9.505         kN

 Plates

 Allowed Surface Pressure                       pG =     490             N/mm^2
 Surface Pressure                                p =     354             N/mm^2
 Force that the Plates Carry                   FBT =       0.000         kN
 Clamping Force                                FKl =      41.890         kN
 Necessary Clamping Force                   Fklerf =      19.048         kN
==============================================================================
                       SAFETIES
==============================================================================
 Dynamic Safety                                 SD =         -
 Static Safety                                  SF =       1.671
 Safety Against Shear                           SA =      25.050
 Safety against Tensile && Shear                SC =       2.782
 Safety Against Surface Pressure                SP =       1.385
 Safety of Seal Function of Connection          SM =       1.000
 Safety Against Shear of Thread             Ssmeff =       1.434
==============================================================================